/*!
    \file  readme.txt
    \brief description of DAC0_output_voltage example
*/

/*
    Copyright (C) 2017 GigaDevice

    2014-12-26, V1.0.0, platform GD32F1x0(x=3,5)
    2016-01-15, V2.0.0, platform GD32F1x0(x=3,5,7,9)
    2016-04-30, V3.0.0, firmware update for GD32F1x0(x=3,5,7,9)
    2017-06-19, V3.1.0, firmware update for GD32F1x0(x=3,5,7,9)
*/

  This example is based on the GD32150R-EVAL/GD32190R-EVAL board, it shows how to use
DAC0 to generate the voltage on DAC channel output.The DAC channel output pin is configured PA4.
DAC0 channel is configured to have an output voltage of VREF/2.