#

##

##

    µVision Build Log
    Project:
    E:\HHD32F0xx_Library_Examples_v20161108\HHD32F0xx_Examples\UART\demo.uvproj
    Project File Date:  03/17/2017

    Output:
    Load "E:\\HHD32F0xx_Library_Examples_v20161108\\HHD32F0xx_Examples\\UART\\myapp\\obj\\demo.AXF"
    Set JLink Project File to "E:\HHD32F0xx_Library_Examples_v20161108\HHD32F0xx_Examples\UART\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled Dec  6 2011 18:57:44
    Hardware: V8.00
    Feature(s) : RDI,FlashDL,FlasGDBFULLash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: Cortex-M0
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 0, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 200 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    Application running ...
    Build target 'Run In Flash'
    compiling core_cm0.c...
    compiling system_hhd32f0xx.c...
    compiling hhd_uart.c...
    compiling hhd_sys.c...
    assembling startup_hhd32F0xx_s.s...
    compiling main.c...
    myapp\src\main.c(59): warning:  #111-D: statement is unreachable
    myapp\src\main.c:       UART_Close(UART0);
    myapp\src\main.c:       ^
    myapp\src\main.c: myapp\src\main.c: 1 warning, 0 errors
    linking...
    Program Size: Code=2676 RO-data=224 RW-data=8 ZI-data=864
    FromELF: creating hex file...
    ".\myapp\obj\demo.axf" - 0 Error(s), 1 Warning(s).
    Load "E:\\HHD32F0xx_Library_Examples_v20161108\\HHD32F0xx_Examples\\UART\\myapp\\obj\\demo.AXF"
    Set JLink Project File to "E:\HHD32F0xx_Library_Examples_v20161108\HHD32F0xx_Examples\UART\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled Dec  6 2011 18:57:44
    Hardware: V8.00
    Feature(s) : RDI,FlashDL,FlasGDBFULLash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: Cortex-M0
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 0, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 4
    Software-Breakpoints: 2048
    Watchpoints:          2
    JTAG speed: 200 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    * JLink Info: Found SWD-DP with ID 0x0BB11477
    * JLink Info:   FPUnit: 4 code (BP) slots and 0 literal slots
    Application running ...