Static Call Graph - [.\myapp\obj\demo.axf]

# Static Call Graph for image .\myapp\obj\demo.axf

#<CALLGRAPH># ARM Linker, 5060422: Last Updated: Tue May 01 19:14:10 2018

### Maximum Stack Usage = 96 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

ADC_IRQHandler_Process ⇒ UIP_SendMessage ⇒ UIP_SetEvent ⇒ uipGetNextPriority

### Functions with no stack information

- __user_initial_stackheap
- uipDisableAllInterrupts
- uipIntMaskStateRestore
- uipPendSVHandler

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- SVC_Handler ⇒ SVC_Handler

  ### Function Pointers

  - ADC_IRQHandler from chip_uip_interrupt.o(i.ADC_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - ADC_IRQHandler_Process from demo.o(i.ADC_IRQHandler_Process) referenced 2 times from app_int_cfg.o(.data)
  - AppIdleTask from demo.o(i.AppIdleTask) referenced 2 times from app_cfg.o(.data)
  - BOD_IRQHandler from chip_uip_interrupt.o(i.BOD_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - Chip_HHD32_ADC_ISR_Handler_Callback from demo.o(i.Chip_HHD32_ADC_ISR_Handler_Callback) referenced 2 times from app_int_cfg.o(.data)
  - GPIOA_IRQHandler from chip_uip_interrupt.o(i.GPIOA_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - GPIOB_IRQHandler from chip_uip_interrupt.o(i.GPIOB_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - GPIOC_IRQHandler from chip_uip_interrupt.o(i.GPIOC_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - HardFault_Handler from startup_hhd32f0xx_s.o(.text) referenced from startup_hhd32f0xx_s.o(RESET)
  - NMI_Handler from startup_hhd32f0xx_s.o(.text) referenced from startup_hhd32f0xx_s.o(RESET)
  - PWM_FAULT_IRQHandler from chip_uip_interrupt.o(i.PWM_FAULT_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - PWM_TIMER_IRQHandler from chip_uip_interrupt.o(i.PWM_TIMER_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - RTC_IRQHandler from chip_uip_interrupt.o(i.RTC_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - Reset_Handler from startup_hhd32f0xx_s.o(.text) referenced from startup_hhd32f0xx_s.o(RESET)
  - SPI_IRQHandler from chip_uip_interrupt.o(i.SPI_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - SVC_Handler from startup_hhd32f0xx_s.o(.text) referenced from startup_hhd32f0xx_s.o(RESET)
  - TASK_0 from demo.o(i.TASK_0) referenced 2 times from app_cfg.o(.data)
  - TASK_1 from demo.o(i.TASK_1) referenced 2 times from app_cfg.o(.data)
  - TASK_2 from demo.o(i.TASK_2) referenced 2 times from app_cfg.o(.data)
  - TASK_3 from demo.o(i.TASK_3) referenced 2 times from app_cfg.o(.data)
  - TASK_4 from demo.o(i.TASK_4) referenced 2 times from app_cfg.o(.data)
  - TIMER16_0_IRQHandler from chip_uip_interrupt.o(i.TIMER16_0_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - TIMER16_1_IRQHandler from chip_uip_interrupt.o(i.TIMER16_1_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - TIMER16_2_IRQHandler from chip_uip_interrupt.o(i.TIMER16_2_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - TIMER16_3_IRQHandler from chip_uip_interrupt.o(i.TIMER16_3_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - TWS_IRQHandler from chip_uip_interrupt.o(i.TWS_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - UART0_IRQHandler from chip_uip_interrupt.o(i.UART0_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - UART1_IRQHandler from chip_uip_interrupt.o(i.UART1_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - WAKEUP_IRQHandler from chip_uip_interrupt.o(i.WAKEUP_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - WDT_IRQHandler from chip_uip_interrupt.o(i.WDT_IRQHandler) referenced from startup_hhd32f0xx_s.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_hhd32f0xx_s.o(.text)
  - uipPendSVHandler from uip_kernel_isr_cm.o(CODE) referenced from startup_hhd32f0xx_s.o(RESET)
  - uipSystemCounterHandler from uip_kernel_time.o(i.uipSystemCounterHandler) referenced from startup_hhd32f0xx_s.o(RESET)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 52 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 44 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ StartOS ⇒ uipAppInitialize ⇒ uipTaskInitialize
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup_hhd32f0xx_s.o(.text))
  [Address Reference Count : 1]

  - startup_hhd32f0xx_s.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_hhd32f0xx_s.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_hhd32f0xx_s.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_hhd32f0xx_s.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_hhd32f0xx_s.o(.text), UNUSED)
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_hhd32f0xx_s.o(.text), UNUSED)
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_hhd32f0xx_s.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 20 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text))
  [Called By]

  - >> ADC_Init
  - >> SystemCoreClockUpdate

  __aeabi_idiv (Thumb, 0 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_idivmod (Thumb, 326 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 62 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 16 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  - >> _call_atexit_fns (Weak Reference)
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  uipDisableAllInterrupts (Thumb, 0 bytes, Stack size unknown bytes, uip_kernel_isr_cm.o(CODE))
  [Called By]

  - >> UIP_WaitEvent
  - >> UIP_TerminateTask
  - >> UIP_SetEvent
  - >> UIP_SendMessage
  - >> UIP_ReleaseResource
  - >> UIP_ReceiveMessage
  - >> UIP_GetResource
  - >> UIP_ClearEvent
  - >> StartOS
  - >> UIP_ActivateTask
  - >> uipInterruptServiceEngine

  uipIntMaskStateRestore (Thumb, 0 bytes, Stack size unknown bytes, uip_kernel_isr_cm.o(CODE))
  [Called By]

  - >> UIP_WaitEvent
  - >> UIP_TerminateTask
  - >> UIP_SetEvent
  - >> UIP_SendMessage
  - >> UIP_ReleaseResource
  - >> UIP_ReceiveMessage
  - >> UIP_GetResource
  - >> UIP_ClearEvent
  - >> StartOS
  - >> UIP_ActivateTask
  - >> uipInterruptServiceEngine

  uipPendSVHandler (Thumb, 0 bytes, Stack size unknown bytes, uip_kernel_isr_cm.o(CODE))
  [Stack]

  - Max Depth = 4 + Unknown Stack Size
  - Call Chain = uipPendSVHandler ⇒ uipPreContexSwitch
  [Calls]
  - >> uipPreContexSwitch
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  ADC_EnableConversionInt (Thumb, 6 bytes, Stack size 0 bytes, hhd_adc.o(i.ADC_EnableConversionInt))
  [Called By]

  - >> TASK_0

  ADC_GetConversionData (Thumb, 24 bytes, Stack size 0 bytes, hhd_adc.o(i.ADC_GetConversionData))
  [Called By]

  - >> ADC_IRQHandler_Process

  ADC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.ADC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = ADC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  ADC_IRQHandler_Process (Thumb, 34 bytes, Stack size 24 bytes, demo.o(i.ADC_IRQHandler_Process))
  [Stack]

  - Max Depth = 96 + Unknown Stack Size
  - Call Chain = ADC_IRQHandler_Process ⇒ UIP_SendMessage ⇒ UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_SendMessage
  - >> ADC_GetConversionData
  [Address Reference Count : 1]
  - app_int_cfg.o(.data)

  ADC_Init (Thumb, 160 bytes, Stack size 16 bytes, hhd_adc.o(i.ADC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = ADC_Init
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> TASK_0

  ADC_SetTrigger (Thumb, 64 bytes, Stack size 8 bytes, hhd_adc.o(i.ADC_SetTrigger))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_SetTrigger
  [Called By]
  - >> TASK_0

  ADC_SetupChannels (Thumb, 66 bytes, Stack size 8 bytes, hhd_adc.o(i.ADC_SetupChannels))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_SetupChannels
  [Called By]
  - >> TASK_0

  AppIdleTask (Thumb, 40 bytes, Stack size 0 bytes, demo.o(i.AppIdleTask))
  [Address Reference Count : 1]

  - app_cfg.o(.data)

  BOD_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.BOD_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = BOD_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  Chip_HHD32_ADC_ISR_Handler_Callback (Thumb, 6 bytes, Stack size 0 bytes, demo.o(i.Chip_HHD32_ADC_ISR_Handler_Callback))
  [Address Reference Count : 1]

  - app_int_cfg.o(.data)

  GPIOA_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.GPIOA_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = GPIOA_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  GPIOB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.GPIOB_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = GPIOB_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  GPIOC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.GPIOC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = GPIOC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  Hardware_Init (Thumb, 2 bytes, Stack size 0 bytes, hardware_init.o(i.Hardware_Init))
  [Called By]

  - >> main

  InterruptHandler (Thumb, 80 bytes, Stack size 32 bytes, chip_uip_interrupt.o(i.InterruptHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = InterruptHandler
  [Called By]
  - >> uipInterruptHandlingCallback

  Kernel_System_Tick_Init (Thumb, 46 bytes, Stack size 0 bytes, hardware_init.o(i.Kernel_System_Tick_Init))
  [Called By]

  - >> uipAppInitialize

  PWM_FAULT_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.PWM_FAULT_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = PWM_FAULT_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  PWM_TIMER_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.PWM_TIMER_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = PWM_TIMER_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  RTC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.RTC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = RTC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  SPI_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.SPI_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = SPI_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  SYS_SystemInitial (Thumb, 40 bytes, Stack size 8 bytes, hhd_sys.o(i.SYS_SystemInitial))
  [Stack]

  - Max Depth = 24
  - Call Chain = SYS_SystemInitial ⇒ SystemInit ⇒ SystemCoreClockUpdate
  [Calls]
  - >> SystemInit
  [Called By]
  - >> TASK_0
  - >> main

  StartOS (Thumb, 38 bytes, Stack size 16 bytes, uip_kernel_common.o(i.StartOS))
  [Stack]

  - Max Depth = 44 + Unknown Stack Size
  - Call Chain = StartOS ⇒ uipAppInitialize ⇒ uipTaskInitialize
  [Calls]
  - >> uipAppInitialize
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  - >> uipKernelInitialize
  [Called By]
  - >> main

  SystemCoreClockUpdate (Thumb, 92 bytes, Stack size 8 bytes, system_hhd32f0xx.o(i.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemCoreClockUpdate
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> TASK_0
  - >> SystemInit

  SystemInit (Thumb, 8 bytes, Stack size 8 bytes, system_hhd32f0xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemInit ⇒ SystemCoreClockUpdate
  [Calls]
  - >> SystemCoreClockUpdate
  [Called By]
  - >> SYS_SystemInitial

  TASK_0 (Thumb, 96 bytes, Stack size 0 bytes, demo.o(i.TASK_0))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = TASK_0 ⇒ UIP_WaitEvent ⇒ uipGetNextTask
  [Calls]
  - >> UIP_WaitEvent
  - >> UIP_ClearEvent
  - >> delay1us
  - >> UartStdOutInit
  - >> ADC_SetupChannels
  - >> ADC_SetTrigger
  - >> ADC_Init
  - >> ADC_EnableConversionInt
  - >> SYS_SystemInitial
  - >> SystemCoreClockUpdate
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_1 (Thumb, 20 bytes, Stack size 0 bytes, demo.o(i.TASK_1))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = TASK_1 ⇒ UIP_WaitEvent ⇒ uipGetNextTask
  [Calls]
  - >> UIP_WaitEvent
  - >> UIP_ClearEvent
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_2 (Thumb, 34 bytes, Stack size 0 bytes, demo.o(i.TASK_2))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = TASK_2 ⇒ UIP_ReleaseResource ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_WaitEvent
  - >> UIP_ReleaseResource
  - >> UIP_GetResource
  - >> UIP_ClearEvent
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_3 (Thumb, 28 bytes, Stack size 0 bytes, demo.o(i.TASK_3))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = TASK_3 ⇒ UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource
  - >> UIP_GetResource
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_4 (Thumb, 16 bytes, Stack size 16 bytes, demo.o(i.TASK_4))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = TASK_4 ⇒ UIP_ReceiveMessage
  [Calls]
  - >> UIP_TerminateTask
  - >> UIP_ReceiveMessage
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TIMER16_0_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIMER16_0_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIMER16_0_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  TIMER16_1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIMER16_1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIMER16_1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  TIMER16_2_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIMER16_2_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIMER16_2_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  TIMER16_3_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIMER16_3_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIMER16_3_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  TWS_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TWS_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TWS_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  UART0_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.UART0_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = UART0_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  UART1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.UART1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = UART1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  UIP_ActivateTask (Thumb, 226 bytes, Stack size 16 bytes, uip_kernel_task.o(i.UIP_ActivateTask))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = UIP_ActivateTask
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> UIP_SendMessage
  - >> uipAlarmHandler

  UIP_ClearEvent (Thumb, 74 bytes, Stack size 16 bytes, uip_kernel_event.o(i.UIP_ClearEvent))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = UIP_ClearEvent
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_2
  - >> TASK_1
  - >> TASK_0

  UIP_GetResource (Thumb, 158 bytes, Stack size 24 bytes, uip_kernel_resource.o(i.UIP_GetResource))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = UIP_GetResource
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_3
  - >> TASK_2

  UIP_ReceiveMessage (Thumb, 206 bytes, Stack size 32 bytes, uip_kernel_message.o(i.UIP_ReceiveMessage))
  [Stack]

  - Max Depth = 32 + Unknown Stack Size
  - Call Chain = UIP_ReceiveMessage
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_4

  UIP_ReleaseResource (Thumb, 264 bytes, Stack size 32 bytes, uip_kernel_resource.o(i.UIP_ReleaseResource))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = UIP_ReleaseResource ⇒ uipGetNextPriority
  [Calls]
  - >> uipGetNextPriority
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_3
  - >> TASK_2

  UIP_SendMessage (Thumb, 268 bytes, Stack size 32 bytes, uip_kernel_message.o(i.UIP_SendMessage))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = UIP_SendMessage ⇒ UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_SetEvent
  - >> UIP_ActivateTask
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> ADC_IRQHandler_Process

  UIP_SetEvent (Thumb, 268 bytes, Stack size 32 bytes, uip_kernel_event.o(i.UIP_SetEvent))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> uipGetNextPriority
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> UIP_SendMessage
  - >> TASK_3
  - >> uipAlarmHandler

  UIP_TerminateTask (Thumb, 244 bytes, Stack size 16 bytes, uip_kernel_task.o(i.UIP_TerminateTask))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = UIP_TerminateTask ⇒ uipGetNextTask
  [Calls]
  - >> uipGetNextTask
  - >> uipClearPrioGrpAndArrayBit
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  - >> uipTaskStackInit
  [Called By]
  - >> TASK_4

  UIP_WaitEvent (Thumb, 128 bytes, Stack size 16 bytes, uip_kernel_event.o(i.UIP_WaitEvent))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = UIP_WaitEvent ⇒ uipGetNextTask
  [Calls]
  - >> uipGetNextTask
  - >> uipClearPrioGrpAndArrayBit
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_2
  - >> TASK_1
  - >> TASK_0

  UartStdOutInit (Thumb, 34 bytes, Stack size 0 bytes, uart_stdout.o(i.UartStdOutInit))
  [Called By]

  - >> TASK_0

  WAKEUP_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.WAKEUP_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = WAKEUP_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  WDT_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.WDT_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = WDT_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  _sys_exit (Thumb, 4 bytes, Stack size 0 bytes, retarget.o(i._sys_exit))
  [Called By]

  - >> __rt_exit_exit

  delay1us (Thumb, 12 bytes, Stack size 0 bytes, demo.o(i.delay1us))
  [Called By]

  - >> TASK_0

  main (Thumb, 26 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 44 + Unknown Stack Size
  - Call Chain = main ⇒ StartOS ⇒ uipAppInitialize ⇒ uipTaskInitialize
  [Calls]
  - >> StartOS
  - >> Hardware_Init
  - >> SYS_SystemInitial
  [Called By]
  - >> __rt_entry_main

  uipAlarmHandler (Thumb, 118 bytes, Stack size 16 bytes, uip_kernel_time.o(i.uipAlarmHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = uipAlarmHandler ⇒ UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_SetEvent
  - >> UIP_ActivateTask
  [Called By]
  - >> uipSystemCounterHandler

  uipAlarmInitialize (Thumb, 34 bytes, Stack size 0 bytes, uip_kernel_common.o(i.uipAlarmInitialize))
  [Called By]

  - >> uipAppInitialize

  uipAppInitialize (Thumb, 62 bytes, Stack size 8 bytes, demo.o(i.uipAppInitialize))
  [Stack]

  - Max Depth = 28
  - Call Chain = uipAppInitialize ⇒ uipTaskInitialize
  [Calls]
  - >> uipTaskInitialize
  - >> uipResInitialize
  - >> uipMsgInitialize
  - >> uipAlarmInitialize
  - >> Kernel_System_Tick_Init
  [Called By]
  - >> StartOS

  uipClearPrioGrpAndArrayBit (Thumb, 108 bytes, Stack size 8 bytes, uip_kernel_scheduler.o(i.uipClearPrioGrpAndArrayBit))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipClearPrioGrpAndArrayBit
  [Called By]
  - >> UIP_WaitEvent
  - >> UIP_TerminateTask

  uipGetNextPriority (Thumb, 82 bytes, Stack size 8 bytes, uip_kernel_scheduler.o(i.uipGetNextPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipGetNextPriority
  [Called By]
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource

  uipGetNextTask (Thumb, 126 bytes, Stack size 8 bytes, uip_kernel_scheduler.o(i.uipGetNextTask))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipGetNextTask
  [Called By]
  - >> UIP_WaitEvent
  - >> UIP_TerminateTask
  - >> uipInterruptServiceEngine

  uipInterruptHandlingCallback (Thumb, 20 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.uipInterruptHandlingCallback))
  [Stack]

  - Max Depth = 40
  - Call Chain = uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> InterruptHandler
  [Called By]
  - >> uipInterruptServiceEngine

  uipInterruptServiceEngine (Thumb, 250 bytes, Stack size 8 bytes, uip_kernel_isr_engine.o(i.uipInterruptServiceEngine))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipGetNextTask
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  - >> uipInterruptHandlingCallback
  [Called By]
  - >> WDT_IRQHandler
  - >> WAKEUP_IRQHandler
  - >> UART1_IRQHandler
  - >> UART0_IRQHandler
  - >> TWS_IRQHandler
  - >> TIMER16_3_IRQHandler
  - >> TIMER16_2_IRQHandler
  - >> TIMER16_1_IRQHandler
  - >> TIMER16_0_IRQHandler
  - >> SPI_IRQHandler
  - >> RTC_IRQHandler
  - >> PWM_TIMER_IRQHandler
  - >> PWM_FAULT_IRQHandler
  - >> GPIOC_IRQHandler
  - >> GPIOB_IRQHandler
  - >> GPIOA_IRQHandler
  - >> BOD_IRQHandler
  - >> ADC_IRQHandler

  uipKernelInitialize (Thumb, 182 bytes, Stack size 8 bytes, uip_kernel_common.o(i.uipKernelInitialize))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipKernelInitialize
  [Called By]
  - >> StartOS

  uipMsgInitialize (Thumb, 60 bytes, Stack size 12 bytes, uip_kernel_common.o(i.uipMsgInitialize))
  [Stack]

  - Max Depth = 12
  - Call Chain = uipMsgInitialize
  [Called By]
  - >> uipAppInitialize

  uipPreContexSwitch (Thumb, 80 bytes, Stack size 4 bytes, uip_kernel_scheduler.o(i.uipPreContexSwitch))
  [Stack]

  - Max Depth = 4
  - Call Chain = uipPreContexSwitch
  [Calls]
  - >> uipResetPrioGrpAndArrayBit
  [Called By]
  - >> uipPendSVHandler

  uipResInitialize (Thumb, 74 bytes, Stack size 12 bytes, uip_kernel_common.o(i.uipResInitialize))
  [Stack]

  - Max Depth = 12
  - Call Chain = uipResInitialize
  [Called By]
  - >> uipAppInitialize

  uipResetPrioGrpAndArrayBit (Thumb, 62 bytes, Stack size 0 bytes, uip_kernel_scheduler.o(i.uipResetPrioGrpAndArrayBit))
  [Called By]

  - >> uipPreContexSwitch

  uipSystemCounterHandler (Thumb, 114 bytes, Stack size 16 bytes, uip_kernel_time.o(i.uipSystemCounterHandler))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = uipSystemCounterHandler ⇒ uipAlarmHandler ⇒ UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> uipAlarmHandler
  [Address Reference Count : 1]
  - startup_hhd32f0xx_s.o(RESET)

  uipTaskInitialize (Thumb, 236 bytes, Stack size 20 bytes, uip_kernel_common.o(i.uipTaskInitialize))
  [Stack]

  - Max Depth = 20
  - Call Chain = uipTaskInitialize
  [Calls]
  - >> uipTaskStackInit
  [Called By]
  - >> uipAppInitialize

  uipTaskStackInit (Thumb, 76 bytes, Stack size 0 bytes, uip_kernel_common.o(i.uipTaskStackInit))
  [Called By]

  - >> uipTaskInitialize
  - >> UIP_TerminateTask

  ### Local Symbols

  ### Undefined Global Symbols

  _call_atexit_fns (ARM, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> exit