#

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: ¦ÌVision V5.23.0.0
    Copyright (C) 2017 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: me me, me, LIC=Q7GX7-EJZII-IN2A7-ECWTI-6IJF9-DG5GC

    Tool Versions:
    Toolchain:       MDK-ARM Professional  Version: 5.23
    Toolchain Path:  d:\Keil_v5\ARM\ARMCC\Bin
    C Compiler:      Armcc.exe V5.06 update 4 (build 422)
    Assembler:       Armasm.exe V5.06 update 4 (build 422)
    Linker/Locator:  ArmLink.exe V5.06 update 4 (build 422)
    Library Manager: ArmAr.exe V5.06 update 4 (build 422)
    Hex Converter:   FromElf.exe V5.06 update 4 (build 422)
    CPU DLL:         SARMCM3.DLL V5.23
    Dialog DLL:      DARMCM1.DLL V1.17.0.0
    Target DLL:      UL2CM3.DLL V1.159.7.0
    Dialog DLL:      TARMCM1.DLL V1.12.0.0

    Project:
    D:\HHD32F0xx_library_examples_on_uipkernel\HHD32F0xx_Examples_on_uipkernel\UART_Interrupt_uipkernel\uart_int.uvproj
    Project File Date:  04/26/2018

    Output:
    *** Using Compiler 'V5.06 update 4 (build 422)', folder: 'd:\Keil_v5\ARM\ARMCC\Bin'
    Rebuild target 'Run In RAM'
    compiling core_cm0.c...
    assembling startup_hhd32F0xx_s.s...
    compiling system_hhd32f0xx.c...
    compiling hhd_sys.c...
    compiling hhd_uart.c...
    compiling main.c...
    compiling app_cfg.c...
    compiling demo.c...
    compiling uip_kernel_common.c...
    compiling chip_uip_interrupt.c...
    compiling hardware_init.c...
    assembling uip_kernel_isr_cm.s...
    compiling uip_kernel_event.c...
    compiling uip_kernel_isr_engine.c...
    compiling uip_kernel_message.c...
    compiling uip_kernel_resource.c...
    compiling uip_kernel_scheduler.c...
    compiling uip_kernel_task.c...
    compiling uip_kernel_time.c...
    ..\..\uipkernel\uip_kernel_time.c(98): warning:  #550-D: parameter "Info"  was set but never used
      StatusType UIP_GetAlarmBase(AlarmType AlarmID, AlarmBaseRefType Info)
    ..\..\uipkernel\uip_kernel_time.c: 1 warning, 0 errors
    linking...
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching startup_hhd32f0xx_s.o(STACK).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching app_cfg.o(.data).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_scheduler.o(.data).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching startup_hhd32f0xx_s.o(HEAP).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_common.o(i.uipTaskStackInit).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_common.o(.bss).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching demo.o(i.uipAppInitialize).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_scheduler.o(i.uipGetNextPriority).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_scheduler.o(i.uipPreContexSwitch).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching libspace.o(.bss).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_event.o(i.UIP_ClearEvent).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_isr_cm.o(CODE).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_common.o(i.uipResInitialize).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_scheduler.o(i.uipResetPrioGrpAndArrayBit).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_common.o(i.uipMsgInitialize).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching hardware_init.o(i.Kernel_System_Tick_Init).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching sys_stackheap_outer.o(.text).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching hhd_sys.o(i.SYS_SystemInitial).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.InterruptHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching startup_hhd32f0xx_s.o(.text).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_common.o(i.StartOS).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_common.o(.data).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching demo.o(i.AppIdleTask).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.Chip_UIP_InterruptInit).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching uip_kernel_common.o(i.uipAlarmInitialize).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching hhd_uart.o(i.UART_Send).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching demo.o(i.TASK_2).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching demo.o(i.TASK_3).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.Chip_UIP_InterruptRegisterHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching demo.o(i.TASK_0).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching demo.o(i.TASK_1).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.uipInterruptHandlingCallback).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching hhd_uart.o(i.NVIC_DisableIRQ).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.ADC_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.BOD_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.GPIOA_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.GPIOB_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.GPIOC_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.PWM_FAULT_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.PWM_TIMER_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.RTC_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.SPI_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.TIMER16_0_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.TIMER16_1_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.TIMER16_2_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.TIMER16_3_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.TWS_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.UART0_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.UART1_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.WAKEUP_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.WDT_IRQHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching demo.o(i.TASK_4).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching exit.o(.text).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching sys_exit.o(.text).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching system_hhd32f0xx.o(.data).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching hhd_uart.o(i.UART_EnableInt).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching hardware_init.o(i.Hardware_Init).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching __rtentry2.o(.ARM.Collect$$rtentry$$0000000D).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching libspace.o(.text).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching heapauxi.o(.text).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching rtexit2.o(.ARM.Collect$$rtexit$$00000004).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching chip_uip_interrupt.o(i.Chip_UIP_InterruptNullHandler).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching system_hhd32f0xx.o(i.SystemInit).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching libinit.o(.ARM.Collect$$libinit$$00000000).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching use_no_semi.o(.text).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching libshutdown.o(.ARM.Collect$$libshutdown$$00000000).
    .\myapp\obj\demo.axf: Error: L6406E: No space in execution regions with .ANY selector matching indicate_semi.o(.text).
    .\myapp\obj\demo.axf: Error: L6407E: Sections of aggregate size 0xebc bytes could not fit into .ANY selector(s).
    Not enough information to list image symbols.
    Not enough information to list the image map.
    Finished: 2 information, 0 warning and 68 error messages.
    ".\myapp\obj\demo.axf" - 68 Error(s), 1 Warning(s).
    Target not created.
    Build Time Elapsed:  00:00:03