Static Call Graph - [.\obj\PWM.axf]

# Static Call Graph for image .\obj\PWM.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Fri May 29 16:20:59 2020

### Maximum Stack Usage = 160 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ pre_main_init ⇒ PWM_ConfigOutputChannel ⇒ CLK_GetHCLKFreq ⇒ SystemCoreClockUpdate

### Functions with no stack information

- __user_initial_stackheap
- uipDisableAllInterrupts
- uipIntMaskStateRestore
- uipPendSVHandler

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- SVC_Handler ⇒ SVC_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler

  ### Function Pointers

  - ADC_IRQHandler from chip_uip_interrupt.o(i.ADC_IRQHandler) referenced from startup_n572.o(RESET)
  - APU_IRQHandler from chip_uip_interrupt.o(i.APU_IRQHandler) referenced from startup_n572.o(RESET)
  - AppIdleTask from demo.o(i.AppIdleTask) referenced from app_cfg.o(.data)
  - Chip_N570_PWM_0_ISR_Handler_Callback from app_int_cfg.o(i.Chip_N570_PWM_0_ISR_Handler_Callback) referenced from app_int_cfg.o(.data)
  - EXINT_IRQHandler from chip_uip_interrupt.o(i.EXINT_IRQHandler) referenced from startup_n572.o(RESET)
  - GPAB_IRQHandler from chip_uip_interrupt.o(i.GPAB_IRQHandler) referenced from startup_n572.o(RESET)
  - HardFault_Handler from startup_n572.o(.text) referenced from startup_n572.o(RESET)
  - NMI_Handler from startup_n572.o(.text) referenced from startup_n572.o(RESET)
  - PWM0_IRQHandler from chip_uip_interrupt.o(i.PWM0_IRQHandler) referenced from startup_n572.o(RESET)
  - PWM0_IRQHandler_Process from init.o(i.PWM0_IRQHandler_Process) referenced from app_int_cfg.o(.data)
  - PWRWU_IRQHandler from chip_uip_interrupt.o(i.PWRWU_IRQHandler) referenced from startup_n572.o(RESET)
  - PendSV_Handler from startup_n572.o(.text) referenced from startup_n572.o(RESET)
  - RTC_IRQHandler from chip_uip_interrupt.o(i.RTC_IRQHandler) referenced from startup_n572.o(RESET)
  - Reset_Handler from startup_n572.o(.text) referenced from startup_n572.o(RESET)
  - SPI0_IRQHandler from chip_uip_interrupt.o(i.SPI0_IRQHandler) referenced from startup_n572.o(RESET)
  - SPI1_IRQHandler from chip_uip_interrupt.o(i.SPI1_IRQHandler) referenced from startup_n572.o(RESET)
  - SVC_Handler from startup_n572.o(.text) referenced from startup_n572.o(RESET)
  - SysTick_Handler from startup_n572.o(.text) referenced from startup_n572.o(RESET)
  - TASK_0 from demo.o(i.TASK_0) referenced from app_cfg.o(.data)
  - TASK_1 from demo.o(i.TASK_1) referenced from app_cfg.o(.data)
  - TASK_2 from demo.o(i.TASK_2) referenced from app_cfg.o(.data)
  - TASK_3 from demo.o(i.TASK_3) referenced from app_cfg.o(.data)
  - TASK_4 from demo.o(i.TASK_4) referenced from app_cfg.o(.data)
  - TMR0_IRQHandler from chip_uip_interrupt.o(i.TMR0_IRQHandler) referenced from startup_n572.o(RESET)
  - TMR1_IRQHandler from chip_uip_interrupt.o(i.TMR1_IRQHandler) referenced from startup_n572.o(RESET)
  - TMR2_IRQHandler from chip_uip_interrupt.o(i.TMR2_IRQHandler) referenced from startup_n572.o(RESET)
  - TMRF_IRQHandler from chip_uip_interrupt.o(i.TMRF_IRQHandler) referenced from startup_n572.o(RESET)
  - USBD_IRQHandler from chip_uip_interrupt.o(i.USBD_IRQHandler) referenced from startup_n572.o(RESET)
  - WDT_IRQHandler from chip_uip_interrupt.o(i.WDT_IRQHandler) referenced from startup_n572.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_n572.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 52 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ pre_main_init ⇒ PWM_ConfigOutputChannel ⇒ CLK_GetHCLKFreq ⇒ SystemCoreClockUpdate
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  SH_DoCommand (Thumb, 18 bytes, Stack size 0 bytes, retarget.o(.emb_text))
  [Called By]

  - >> _sys_exit

  __aeabi_memcpy4 (Thumb, 56 bytes, Stack size 0 bytes, rt_memcpy.o(.emb_text))
  [Called By]

  - >> PWM_ConfigOutputChannel

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, rt_memcpy.o(.emb_text), UNUSED)

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup_n572.o(.text))

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n572.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n572.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n572.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n572.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n572.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_n572.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 20 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text))
  [Called By]

  - >> PWM_ConfigOutputChannel
  - >> Kernel_System_Tick_Init
  - >> SystemCoreClockUpdate

  __aeabi_idiv (Thumb, 0 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_idivmod (Thumb, 326 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 62 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 16 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> _call_atexit_fns (Weak Reference)
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  uipDisableAllInterrupts (Thumb, 0 bytes, Stack size unknown bytes, uip_kernel_isr_cm.o(CODE))
  [Called By]

  - >> UIP_WaitEvent
  - >> UIP_TerminateTask
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource
  - >> UIP_ReceiveMessage
  - >> UIP_GetResource
  - >> UIP_ClearEvent
  - >> StartOS
  - >> uipInterruptServiceEngine

  uipIntMaskStateRestore (Thumb, 0 bytes, Stack size unknown bytes, uip_kernel_isr_cm.o(CODE))
  [Called By]

  - >> UIP_WaitEvent
  - >> UIP_TerminateTask
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource
  - >> UIP_ReceiveMessage
  - >> UIP_GetResource
  - >> UIP_ClearEvent
  - >> StartOS
  - >> uipInterruptServiceEngine

  uipPendSVHandler (Thumb, 0 bytes, Stack size unknown bytes, uip_kernel_isr_cm.o(CODE), UNUSED)
  [Calls]

  - >> uipPreContexSwitch

  ADC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.ADC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = ADC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  APU_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.APU_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = APU_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  AppIdleTask (Thumb, 40 bytes, Stack size 0 bytes, demo.o(i.AppIdleTask))
  [Address Reference Count : 1]

  - app_cfg.o(.data)

  CLK_EnableModuleClock (Thumb, 48 bytes, Stack size 16 bytes, clk.o(i.CLK_EnableModuleClock))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLK_EnableModuleClock
  [Calls]
  - >> SYS_Unlock
  - >> SYS_Lock
  [Called By]
  - >> SYS_Init

  CLK_EnableXtalRC (Thumb, 28 bytes, Stack size 16 bytes, clk.o(i.CLK_EnableXtalRC))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLK_EnableXtalRC
  [Calls]
  - >> SYS_Unlock
  - >> SYS_Lock
  [Called By]
  - >> SYS_Init

  CLK_GetHCLKFreq (Thumb, 12 bytes, Stack size 8 bytes, clk.o(i.CLK_GetHCLKFreq))
  [Stack]

  - Max Depth = 24
  - Call Chain = CLK_GetHCLKFreq ⇒ SystemCoreClockUpdate
  [Calls]
  - >> SystemCoreClockUpdate
  [Called By]
  - >> PWM_ConfigOutputChannel

  CLK_GetPLL2ClockFreq (Thumb, 48 bytes, Stack size 0 bytes, clk.o(i.CLK_GetPLL2ClockFreq))
  [Called By]

  - >> SystemCoreClockUpdate

  CLK_SetHCLK (Thumb, 50 bytes, Stack size 16 bytes, clk.o(i.CLK_SetHCLK))
  [Stack]

  - Max Depth = 32
  - Call Chain = CLK_SetHCLK ⇒ SystemCoreClockUpdate
  [Calls]
  - >> SYS_Unlock
  - >> SYS_Lock
  - >> SystemCoreClockUpdate
  [Called By]
  - >> SYS_Init

  CLK_SetModuleClock (Thumb, 122 bytes, Stack size 32 bytes, clk.o(i.CLK_SetModuleClock))
  [Stack]

  - Max Depth = 32
  - Call Chain = CLK_SetModuleClock
  [Calls]
  - >> SYS_Unlock
  - >> SYS_Lock
  [Called By]
  - >> SYS_Init

  CLK_SetPLL1Mode (Thumb, 18 bytes, Stack size 0 bytes, clk.o(i.CLK_SetPLL1Mode))
  [Called By]

  - >> SYS_Init

  CLK_SetPLL2 (Thumb, 30 bytes, Stack size 0 bytes, clk.o(i.CLK_SetPLL2))
  [Called By]

  - >> SYS_Init

  CLK_SetPLL2Mode (Thumb, 18 bytes, Stack size 0 bytes, clk.o(i.CLK_SetPLL2Mode))
  [Called By]

  - >> SYS_Init

  Chip_N570_PWM_0_ISR_Handler_Callback (Thumb, 6 bytes, Stack size 0 bytes, app_int_cfg.o(i.Chip_N570_PWM_0_ISR_Handler_Callback))
  [Address Reference Count : 1]

  - app_int_cfg.o(.data)

  EXINT_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.EXINT_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = EXINT_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  GPAB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.GPAB_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = GPAB_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  Hardware_Init (Thumb, 2 bytes, Stack size 0 bytes, hardware_init.o(i.Hardware_Init))
  [Called By]

  - >> main

  InterruptHandler (Thumb, 80 bytes, Stack size 32 bytes, chip_uip_interrupt.o(i.InterruptHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = InterruptHandler
  [Called By]
  - >> uipInterruptHandlingCallback

  IsDebugFifoEmpty (Thumb, 4 bytes, Stack size 0 bytes, retarget.o(i.IsDebugFifoEmpty))
  [Called By]

  - >> _sys_exit

  Kernel_System_Tick_Init (Thumb, 60 bytes, Stack size 8 bytes, hardware_init.o(i.Kernel_System_Tick_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = Kernel_System_Tick_Init
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> uipAppInitialize

  PWM0_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.PWM0_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = PWM0_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  PWM0_IRQHandler_Process (Thumb, 32 bytes, Stack size 16 bytes, init.o(i.PWM0_IRQHandler_Process))
  [Stack]

  - Max Depth = 16
  - Call Chain = PWM0_IRQHandler_Process
  [Calls]
  - >> PWM_SetCNR
  - >> PWM_SetCMR
  - >> PWM_ClearIntFlag
  [Address Reference Count : 1]
  - app_int_cfg.o(.data)

  PWM_ClearIntFlag (Thumb, 10 bytes, Stack size 0 bytes, pwm.o(i.PWM_ClearIntFlag))
  [Called By]

  - >> PWM0_IRQHandler_Process

  PWM_ConfigOutputChannel (Thumb, 332 bytes, Stack size 120 bytes, pwm.o(i.PWM_ConfigOutputChannel))
  [Stack]

  - Max Depth = 144
  - Call Chain = PWM_ConfigOutputChannel ⇒ CLK_GetHCLKFreq ⇒ SystemCoreClockUpdate
  [Calls]
  - >> CLK_GetHCLKFreq
  - >> __aeabi_uidivmod
  - >> __aeabi_memcpy4
  [Called By]
  - >> pre_main_init

  PWM_EnableOutput (Thumb, 62 bytes, Stack size 0 bytes, pwm.o(i.PWM_EnableOutput))
  [Called By]

  - >> pre_main_init

  PWM_SetCMR (Thumb, 44 bytes, Stack size 0 bytes, pwm.o(i.PWM_SetCMR))
  [Called By]

  - >> PWM0_IRQHandler_Process

  PWM_SetCNR (Thumb, 10 bytes, Stack size 0 bytes, pwm.o(i.PWM_SetCNR))
  [Called By]

  - >> PWM0_IRQHandler_Process

  PWM_Start (Thumb, 10 bytes, Stack size 0 bytes, pwm.o(i.PWM_Start))
  [Called By]

  - >> TASK_0

  PWRWU_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.PWRWU_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = PWRWU_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  RTC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.RTC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = RTC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  SPI0_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.SPI0_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = SPI0_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  SPI1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.SPI1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = SPI1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  SYS_Init (Thumb, 110 bytes, Stack size 8 bytes, init.o(i.SYS_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = SYS_Init ⇒ CLK_SetModuleClock
  [Calls]
  - >> SYS_UnlockReg
  - >> SYS_SetRamWaitSate
  - >> SYS_SetCpuWaiState
  - >> SYS_ResetModule
  - >> SYS_LockReg
  - >> CLK_SetPLL2Mode
  - >> CLK_SetPLL2
  - >> CLK_SetPLL1Mode
  - >> CLK_SetModuleClock
  - >> CLK_SetHCLK
  - >> CLK_EnableXtalRC
  - >> CLK_EnableModuleClock
  - >> SystemCoreClockUpdate
  [Called By]
  - >> pre_main_init

  SYS_Lock (Thumb, 12 bytes, Stack size 0 bytes, sys.o(i.SYS_Lock))
  [Called By]

  - >> SYS_SetRamWaitSate
  - >> SYS_SetCpuWaiState
  - >> SYS_ResetModule
  - >> CLK_SetModuleClock
  - >> CLK_SetHCLK
  - >> CLK_EnableXtalRC
  - >> CLK_EnableModuleClock

  SYS_LockReg (Thumb, 8 bytes, Stack size 0 bytes, sys.o(i.SYS_LockReg))
  [Called By]

  - >> SYS_Init
  - >> pre_main_init

  SYS_ResetModule (Thumb, 64 bytes, Stack size 8 bytes, sys.o(i.SYS_ResetModule))
  [Stack]

  - Max Depth = 8
  - Call Chain = SYS_ResetModule
  [Calls]
  - >> SYS_Unlock
  - >> SYS_Lock
  [Called By]
  - >> SYS_Init

  SYS_SetCpuWaiState (Thumb, 36 bytes, Stack size 8 bytes, sys.o(i.SYS_SetCpuWaiState))
  [Stack]

  - Max Depth = 8
  - Call Chain = SYS_SetCpuWaiState
  [Calls]
  - >> SYS_Unlock
  - >> SYS_Lock
  [Called By]
  - >> SYS_Init

  SYS_SetRamWaitSate (Thumb, 36 bytes, Stack size 8 bytes, sys.o(i.SYS_SetRamWaitSate))
  [Stack]

  - Max Depth = 8
  - Call Chain = SYS_SetRamWaitSate
  [Calls]
  - >> SYS_Unlock
  - >> SYS_Lock
  [Called By]
  - >> SYS_Init

  SYS_Unlock (Thumb, 44 bytes, Stack size 0 bytes, sys.o(i.SYS_Unlock))
  [Called By]

  - >> SYS_SetRamWaitSate
  - >> SYS_SetCpuWaiState
  - >> SYS_ResetModule
  - >> CLK_SetModuleClock
  - >> CLK_SetHCLK
  - >> CLK_EnableXtalRC
  - >> CLK_EnableModuleClock

  SYS_UnlockReg (Thumb, 26 bytes, Stack size 0 bytes, sys.o(i.SYS_UnlockReg))
  [Called By]

  - >> SYS_Init

  StartOS (Thumb, 38 bytes, Stack size 16 bytes, uip_kernel_common.o(i.StartOS))
  [Stack]

  - Max Depth = 44 + Unknown Stack Size
  - Call Chain = StartOS ⇒ uipAppInitialize ⇒ uipTaskInitialize
  [Calls]
  - >> uipAppInitialize
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  - >> uipKernelInitialize
  [Called By]
  - >> main

  SystemCoreClockUpdate (Thumb, 94 bytes, Stack size 16 bytes, system_n572.o(i.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemCoreClockUpdate
  [Calls]
  - >> CLK_GetPLL2ClockFreq
  - >> __aeabi_uidivmod
  [Called By]
  - >> CLK_GetHCLKFreq
  - >> CLK_SetHCLK
  - >> SYS_Init

  TASK_0 (Thumb, 50 bytes, Stack size 0 bytes, demo.o(i.TASK_0))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = TASK_0 ⇒ UIP_WaitEvent ⇒ uipGetNextTask
  [Calls]
  - >> UIP_WaitEvent
  - >> UIP_ClearEvent
  - >> PWM_Start
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_1 (Thumb, 20 bytes, Stack size 0 bytes, demo.o(i.TASK_1))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = TASK_1 ⇒ UIP_WaitEvent ⇒ uipGetNextTask
  [Calls]
  - >> UIP_WaitEvent
  - >> UIP_ClearEvent
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_2 (Thumb, 34 bytes, Stack size 0 bytes, demo.o(i.TASK_2))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = TASK_2 ⇒ UIP_ReleaseResource ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_WaitEvent
  - >> UIP_ReleaseResource
  - >> UIP_GetResource
  - >> UIP_ClearEvent
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_3 (Thumb, 28 bytes, Stack size 0 bytes, demo.o(i.TASK_3))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = TASK_3 ⇒ UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource
  - >> UIP_GetResource
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_4 (Thumb, 16 bytes, Stack size 24 bytes, demo.o(i.TASK_4))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TASK_4 ⇒ UIP_ReceiveMessage
  [Calls]
  - >> UIP_TerminateTask
  - >> UIP_ReceiveMessage
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TMR0_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TMR0_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TMR0_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  TMR1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TMR1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TMR1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  TMR2_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TMR2_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TMR2_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  TMRF_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TMRF_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TMRF_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  UIP_ClearEvent (Thumb, 74 bytes, Stack size 16 bytes, uip_kernel_event.o(i.UIP_ClearEvent))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = UIP_ClearEvent
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_2
  - >> TASK_1
  - >> TASK_0

  UIP_GetResource (Thumb, 158 bytes, Stack size 24 bytes, uip_kernel_resource.o(i.UIP_GetResource))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = UIP_GetResource
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_3
  - >> TASK_2

  UIP_ReceiveMessage (Thumb, 206 bytes, Stack size 32 bytes, uip_kernel_message.o(i.UIP_ReceiveMessage))
  [Stack]

  - Max Depth = 32 + Unknown Stack Size
  - Call Chain = UIP_ReceiveMessage
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_4

  UIP_ReleaseResource (Thumb, 252 bytes, Stack size 32 bytes, uip_kernel_resource.o(i.UIP_ReleaseResource))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = UIP_ReleaseResource ⇒ uipGetNextPriority
  [Calls]
  - >> uipGetNextPriority
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_3
  - >> TASK_2

  UIP_SetEvent (Thumb, 268 bytes, Stack size 32 bytes, uip_kernel_event.o(i.UIP_SetEvent))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> uipGetNextPriority
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_3

  UIP_TerminateTask (Thumb, 244 bytes, Stack size 16 bytes, uip_kernel_task.o(i.UIP_TerminateTask))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = UIP_TerminateTask ⇒ uipGetNextTask
  [Calls]
  - >> uipGetNextTask
  - >> uipClearPrioGrpAndArrayBit
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  - >> uipTaskStackInit
  [Called By]
  - >> TASK_4

  UIP_WaitEvent (Thumb, 128 bytes, Stack size 16 bytes, uip_kernel_event.o(i.UIP_WaitEvent))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = UIP_WaitEvent ⇒ uipGetNextTask
  [Calls]
  - >> uipGetNextTask
  - >> uipClearPrioGrpAndArrayBit
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_2
  - >> TASK_1
  - >> TASK_0

  USBD_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.USBD_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = USBD_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  WDT_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.WDT_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = WDT_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_n572.o(RESET)

  _sys_exit (Thumb, 28 bytes, Stack size 0 bytes, retarget.o(i._sys_exit))
  [Calls]

  - >> IsDebugFifoEmpty
  - >> SH_DoCommand
  [Called By]
  - >> __rt_exit_exit

  main (Thumb, 26 bytes, Stack size 0 bytes, demo.o(i.main))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = main ⇒ pre_main_init ⇒ PWM_ConfigOutputChannel ⇒ CLK_GetHCLKFreq ⇒ SystemCoreClockUpdate
  [Calls]
  - >> pre_main_init
  - >> StartOS
  - >> Hardware_Init
  [Called By]
  - >> __rt_entry_main

  pre_main_init (Thumb, 48 bytes, Stack size 16 bytes, init.o(i.pre_main_init))
  [Stack]

  - Max Depth = 160
  - Call Chain = pre_main_init ⇒ PWM_ConfigOutputChannel ⇒ CLK_GetHCLKFreq ⇒ SystemCoreClockUpdate
  [Calls]
  - >> SYS_LockReg
  - >> PWM_EnableOutput
  - >> PWM_ConfigOutputChannel
  - >> SYS_Init
  [Called By]
  - >> main

  uipAlarmInitialize (Thumb, 34 bytes, Stack size 0 bytes, uip_kernel_common.o(i.uipAlarmInitialize))
  [Called By]

  - >> uipAppInitialize

  uipAppInitialize (Thumb, 62 bytes, Stack size 8 bytes, demo.o(i.uipAppInitialize))
  [Stack]

  - Max Depth = 28
  - Call Chain = uipAppInitialize ⇒ uipTaskInitialize
  [Calls]
  - >> uipTaskInitialize
  - >> uipResInitialize
  - >> uipMsgInitialize
  - >> uipAlarmInitialize
  - >> Kernel_System_Tick_Init
  [Called By]
  - >> StartOS

  uipClearPrioGrpAndArrayBit (Thumb, 108 bytes, Stack size 8 bytes, uip_kernel_scheduler.o(i.uipClearPrioGrpAndArrayBit))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipClearPrioGrpAndArrayBit
  [Called By]
  - >> UIP_WaitEvent
  - >> UIP_TerminateTask

  uipGetNextPriority (Thumb, 82 bytes, Stack size 8 bytes, uip_kernel_scheduler.o(i.uipGetNextPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipGetNextPriority
  [Called By]
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource

  uipGetNextTask (Thumb, 126 bytes, Stack size 8 bytes, uip_kernel_scheduler.o(i.uipGetNextTask))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipGetNextTask
  [Called By]
  - >> UIP_WaitEvent
  - >> UIP_TerminateTask
  - >> uipInterruptServiceEngine

  uipInterruptHandlingCallback (Thumb, 20 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.uipInterruptHandlingCallback))
  [Stack]

  - Max Depth = 40
  - Call Chain = uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> InterruptHandler
  [Called By]
  - >> uipInterruptServiceEngine

  uipInterruptServiceEngine (Thumb, 264 bytes, Stack size 8 bytes, uip_kernel_isr_engine.o(i.uipInterruptServiceEngine))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipGetNextTask
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  - >> uipInterruptHandlingCallback
  [Called By]
  - >> WDT_IRQHandler
  - >> USBD_IRQHandler
  - >> TMRF_IRQHandler
  - >> TMR2_IRQHandler
  - >> TMR1_IRQHandler
  - >> TMR0_IRQHandler
  - >> SPI1_IRQHandler
  - >> SPI0_IRQHandler
  - >> RTC_IRQHandler
  - >> PWRWU_IRQHandler
  - >> PWM0_IRQHandler
  - >> GPAB_IRQHandler
  - >> EXINT_IRQHandler
  - >> APU_IRQHandler
  - >> ADC_IRQHandler

  uipKernelInitialize (Thumb, 182 bytes, Stack size 8 bytes, uip_kernel_common.o(i.uipKernelInitialize))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipKernelInitialize
  [Called By]
  - >> StartOS

  uipMsgInitialize (Thumb, 60 bytes, Stack size 12 bytes, uip_kernel_common.o(i.uipMsgInitialize))
  [Stack]

  - Max Depth = 12
  - Call Chain = uipMsgInitialize
  [Called By]
  - >> uipAppInitialize

  uipPreContexSwitch (Thumb, 68 bytes, Stack size 4 bytes, uip_kernel_scheduler.o(i.uipPreContexSwitch), UNUSED)
  [Calls]

  - >> uipResetPrioGrpAndArrayBit
  [Called By]
  - >> uipPendSVHandler

  uipResInitialize (Thumb, 74 bytes, Stack size 12 bytes, uip_kernel_common.o(i.uipResInitialize))
  [Stack]

  - Max Depth = 12
  - Call Chain = uipResInitialize
  [Called By]
  - >> uipAppInitialize

  uipResetPrioGrpAndArrayBit (Thumb, 62 bytes, Stack size 0 bytes, uip_kernel_scheduler.o(i.uipResetPrioGrpAndArrayBit), UNUSED)
  [Called By]

  - >> uipPreContexSwitch

  uipTaskInitialize (Thumb, 236 bytes, Stack size 20 bytes, uip_kernel_common.o(i.uipTaskInitialize))
  [Stack]

  - Max Depth = 20
  - Call Chain = uipTaskInitialize
  [Calls]
  - >> uipTaskStackInit
  [Called By]
  - >> uipAppInitialize

  uipTaskStackInit (Thumb, 76 bytes, Stack size 0 bytes, uip_kernel_common.o(i.uipTaskStackInit))
  [Called By]

  - >> uipTaskInitialize
  - >> UIP_TerminateTask

  ### Local Symbols

  ### Undefined Global Symbols

  _call_atexit_fns (ARM, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> exit