


ARM Macro Assembler    Page 1 


    1 00000000         ;/******************************************************
                       ************************
    2 00000000         ; * @file     startup_N572.s
    3 00000000         ; * @version  V1.00
    4 00000000         ; * $Revision: 3 $
    5 00000000         ; * $Date: 14/07/17 11:28a $ 
    6 00000000         ; * @brief    CMSIS ARM Cortex-M0 Core Device Startup Fi
                       le
    7 00000000         ; *
    8 00000000         ; * @note
    9 00000000         ; * Copyright (C) 2014 Nuvoton Technology Corp. All righ
                       ts reserved.
   10 00000000         ;*******************************************************
                       **********************/  
   11 00000000         
   12 00000000         ; <h> Stack Configuration
   13 00000000         ;   <o> Stack Size (in Bytes) <0x0-0xFFFFFFFF:8>
   14 00000000         ; </h>
   15 00000000         
   16 00000000 00000100 
                       Stack_Size
                               EQU              0x00000100
   17 00000000         
   18 00000000                 AREA             STACK, NOINIT, READWRITE, ALIGN
=3
   19 00000000         Stack_Mem
                               SPACE            Stack_Size
   20 00000100         __initial_sp
   21 00000100         
   22 00000100         
   23 00000100         ; <h> Heap Configuration
   24 00000100         ;   <o>  Heap Size (in Bytes) <0x0-0xFFFFFFFF:8>
   25 00000100         ; </h>
   26 00000100         
   27 00000100 00000000 
                       Heap_Size
                               EQU              0x00000000
   28 00000100         
   29 00000100                 AREA             HEAP, NOINIT, READWRITE, ALIGN=
3
   30 00000000         __heap_base
   31 00000000         Heap_Mem
                               SPACE            Heap_Size
   32 00000000         __heap_limit
   33 00000000         
   34 00000000         
   35 00000000         PRESERVE8
   36 00000000                 THUMB
   37 00000000         
   38 00000000         
   39 00000000         ; Vector Table Mapped to Address 0 at Reset
   40 00000000         
   41 00000000                 AREA             RESET, DATA, READONLY
   42 00000000                 EXPORT           __Vectors
   43 00000000         
   44 00000000 00000000 
                       __Vectors
                               DCD              __initial_sp ; Top of Stack
   45 00000004 00000000        DCD              Reset_Handler ; Reset Handler



ARM Macro Assembler    Page 2 


   46 00000008 00000000        DCD              NMI_Handler ; NMI Handler
   47 0000000C 00000000        DCD              HardFault_Handler ; Hard Fault 
                                                            Handler
   48 00000010 00000000        DCD              0           ; Reserved
   49 00000014 00000000        DCD              0           ; Reserved
   50 00000018 00000000        DCD              0           ; Reserved
   51 0000001C 00000000        DCD              0           ; Reserved
   52 00000020 00000000        DCD              0           ; Reserved
   53 00000024 00000000        DCD              0           ; Reserved
   54 00000028 00000000        DCD              0           ; Reserved
   55 0000002C 00000000        DCD              SVC_Handler ; SVCall Handler
   56 00000030 00000000        DCD              0           ; Reserved
   57 00000034 00000000        DCD              0           ; Reserved
   58 00000038 00000000        DCD              PendSV_Handler ; PendSV Handler
                                                            
   59 0000003C 00000000        DCD              SysTick_Handler 
                                                            ; SysTick Handler
   60 00000040         ; External Interrupts
   61 00000040         ; maximum of 32 External Interrupts are possible
   62 00000040 00000000        DCD              WDT_IRQHandler
   63 00000044 00000000        DCD              APU_IRQHandler
   64 00000048 00000000        DCD              ADC_IRQHandler
   65 0000004C 00000000        DCD              EXINT_IRQHandler
   66 00000050 00000000        DCD              USBD_IRQHandler
   67 00000054 00000000        DCD              TMR0_IRQHandler
   68 00000058 00000000        DCD              TMR1_IRQHandler
   69 0000005C 00000000        DCD              TMR2_IRQHandler
   70 00000060 00000000        DCD              GPAB_IRQHandler
   71 00000064 00000000        DCD              SPI0_IRQHandler
   72 00000068 00000000        DCD              PWM0_IRQHandler
   73 0000006C 00000000        DCD              SPI1_IRQHandler
   74 00000070 00000000        DCD              TMRF_IRQHandler
   75 00000074 00000000        DCD              RTC_IRQHandler
   76 00000078 00000000        DCD              PWRWU_IRQHandler
   77 0000007C                 AREA             |.text|, CODE, READONLY
   78 00000000         
   79 00000000         
   80 00000000         
   81 00000000         ; Reset Handler
   82 00000000         
   83 00000000         Reset_Handler
                               PROC
   84 00000000                 EXPORT           Reset_Handler             [WEAK
]
   85 00000000                 IMPORT           __main
   86 00000000 4806            LDR              R0, =__main
   87 00000002 4700            BX               R0
   88 00000004                 ENDP
   89 00000004         
   90 00000004         
   91 00000004         ; Dummy Exception Handlers (infinite loops which can be 
                       modified)                
   92 00000004         
   93 00000004         NMI_Handler
                               PROC
   94 00000004                 EXPORT           NMI_Handler               [WEAK
]
   95 00000004 E7FE            B                .
   96 00000006                 ENDP



ARM Macro Assembler    Page 3 


   98 00000006         HardFault_Handler
                               PROC
   99 00000006                 EXPORT           HardFault_Handler         [WEAK
]
  100 00000006 E7FE            B                .
  101 00000008                 ENDP
  102 00000008         SVC_Handler
                               PROC
  103 00000008                 EXPORT           SVC_Handler               [WEAK
]
  104 00000008 E7FE            B                .
  105 0000000A                 ENDP
  106 0000000A         PendSV_Handler
                               PROC
  107 0000000A                 EXPORT           PendSV_Handler            [WEAK
]
  108 0000000A E7FE            B                .
  109 0000000C                 ENDP
  110 0000000C         SysTick_Handler
                               PROC
  111 0000000C                 EXPORT           SysTick_Handler           [WEAK
]
  112 0000000C E7FE            B                .
  113 0000000E                 ENDP
  114 0000000E         Default_Handler
                               PROC
  115 0000000E         
  116 0000000E                 EXPORT           WDT_IRQHandler     [WEAK]
  117 0000000E                 EXPORT           APU_IRQHandler     [WEAK]
  118 0000000E                 EXPORT           ADC_IRQHandler     [WEAK]
  119 0000000E                 EXPORT           EXINT_IRQHandler    [WEAK]
  120 0000000E                 EXPORT           USBD_IRQHandler     [WEAK]
  121 0000000E                 EXPORT           TMR0_IRQHandler     [WEAK]
  122 0000000E                 EXPORT           TMR1_IRQHandler     [WEAK]
  123 0000000E                 EXPORT           TMR2_IRQHandler     [WEAK]
  124 0000000E                 EXPORT           GPAB_IRQHandler     [WEAK]
  125 0000000E                 EXPORT           SPI0_IRQHandler     [WEAK]
  126 0000000E                 EXPORT           PWM0_IRQHandler     [WEAK]
  127 0000000E                 EXPORT           SPI1_IRQHandler     [WEAK]
  128 0000000E                 EXPORT           TMRF_IRQHandler     [WEAK]
  129 0000000E                 EXPORT           RTC_IRQHandler            [WEAK
]
  130 0000000E                 EXPORT           PWRWU_IRQHandler          [WEAK
]
  131 0000000E         
  132 0000000E         WDT_IRQHandler
  133 0000000E         APU_IRQHandler
  134 0000000E         ADC_IRQHandler
  135 0000000E         EXINT_IRQHandler
  136 0000000E         USBD_IRQHandler
  137 0000000E         TMR0_IRQHandler
  138 0000000E         TMR1_IRQHandler
  139 0000000E         TMR2_IRQHandler
  140 0000000E         GPAB_IRQHandler
  141 0000000E         SPI0_IRQHandler
  142 0000000E         PWM0_IRQHandler
  143 0000000E         SPI1_IRQHandler
  144 0000000E         TMRF_IRQHandler
  145 0000000E         RTC_IRQHandler



ARM Macro Assembler    Page 4 


  146 0000000E         PWRWU_IRQHandler
  147 0000000E         
  148 0000000E E7FE            B                .
  149 00000010         
  150 00000010                 ENDP
  151 00000010         
  152 00000010         
  153 00000010                 ALIGN
  154 00000010         
  155 00000010         
  156 00000010         ; User Initial Stack & Heap
  157 00000010         
  158 00000010                 IF               :DEF:__MICROLIB
  165 00000010         
  166 00000010                 IMPORT           __use_two_region_memory
  167 00000010                 EXPORT           __user_initial_stackheap
  168 00000010         __user_initial_stackheap
  169 00000010         
  170 00000010 4803            LDR              R0, =  Heap_Mem
  171 00000012 4904            LDR              R1, =(Stack_Mem + Stack_Size)
  172 00000014 4A02            LDR              R2, = (Heap_Mem +  Heap_Size)
  173 00000016 4B04            LDR              R3, = Stack_Mem
  174 00000018 4770            BX               LR
  175 0000001A         
  176 0000001A 00 00           ALIGN
  177 0000001C         
  178 0000001C                 ENDIF
  179 0000001C         
  180 0000001C         
  181 0000001C                 END
              00000000 
              00000000 
              00000100 
              00000000 
Command Line: --16 --debug --xref --diag_suppress=9931 --cpu=Cortex-M0 --apcs=i
nterwork --depend=.\obj\startup_n572.d -o.\obj\startup_n572.o -IC:\Keil_v5\ARM\
RV31\INC -IC:\Keil_v5\ARM\CMSIS\Include --predefine="__UVISION_VERSION SETA 527
" --list=.\lst\startup_n572.lst ..\..\..\Library\Device\Nuvoton\N572\Source\ARM
\startup_N572.s



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

STACK 00000000

Symbol: STACK
   Definitions
      At line 18 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      None
Comment: STACK unused
Stack_Mem 00000000

Symbol: Stack_Mem
   Definitions
      At line 19 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 171 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
      At line 173 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

__initial_sp 00000100

Symbol: __initial_sp
   Definitions
      At line 20 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 44 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
Comment: __initial_sp used once
3 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

HEAP 00000000

Symbol: HEAP
   Definitions
      At line 29 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      None
Comment: HEAP unused
Heap_Mem 00000000

Symbol: Heap_Mem
   Definitions
      At line 31 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 170 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
      At line 172 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

PRESERVE8 00000000

Symbol: PRESERVE8
   Definitions
      At line 35 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      None
Comment: PRESERVE8 unused
__heap_base 00000000

Symbol: __heap_base
   Definitions
      At line 30 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      None
Comment: __heap_base unused
__heap_limit 00000000

Symbol: __heap_limit
   Definitions
      At line 32 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      None
Comment: __heap_limit unused
5 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

RESET 00000000

Symbol: RESET
   Definitions
      At line 41 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      None
Comment: RESET unused
__Vectors 00000000

Symbol: __Vectors
   Definitions
      At line 44 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 42 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
Comment: __Vectors used once
2 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

.text 00000000

Symbol: .text
   Definitions
      At line 77 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      None
Comment: .text unused
ADC_IRQHandler 0000000E

Symbol: ADC_IRQHandler
   Definitions
      At line 134 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 64 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 118 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

APU_IRQHandler 0000000E

Symbol: APU_IRQHandler
   Definitions
      At line 133 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 63 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 117 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

Default_Handler 0000000E

Symbol: Default_Handler
   Definitions
      At line 114 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      None
Comment: Default_Handler unused
EXINT_IRQHandler 0000000E

Symbol: EXINT_IRQHandler
   Definitions
      At line 135 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 65 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 119 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

GPAB_IRQHandler 0000000E

Symbol: GPAB_IRQHandler
   Definitions
      At line 140 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start



ARM Macro Assembler    Page 2 Alphabetic symbol ordering
Relocatable symbols

up_N572.s
   Uses
      At line 70 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 124 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

HardFault_Handler 00000006

Symbol: HardFault_Handler
   Definitions
      At line 98 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 47 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 99 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s

NMI_Handler 00000004

Symbol: NMI_Handler
   Definitions
      At line 93 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 46 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 94 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s

PWM0_IRQHandler 0000000E

Symbol: PWM0_IRQHandler
   Definitions
      At line 142 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 72 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 126 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

PWRWU_IRQHandler 0000000E

Symbol: PWRWU_IRQHandler
   Definitions
      At line 146 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 76 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 130 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

PendSV_Handler 0000000A

Symbol: PendSV_Handler
   Definitions



ARM Macro Assembler    Page 3 Alphabetic symbol ordering
Relocatable symbols

      At line 106 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 58 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 107 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

RTC_IRQHandler 0000000E

Symbol: RTC_IRQHandler
   Definitions
      At line 145 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 75 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 129 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

Reset_Handler 00000000

Symbol: Reset_Handler
   Definitions
      At line 83 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 45 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 84 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s

SPI0_IRQHandler 0000000E

Symbol: SPI0_IRQHandler
   Definitions
      At line 141 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 71 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 125 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

SPI1_IRQHandler 0000000E

Symbol: SPI1_IRQHandler
   Definitions
      At line 143 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 73 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 127 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

SVC_Handler 00000008

Symbol: SVC_Handler



ARM Macro Assembler    Page 4 Alphabetic symbol ordering
Relocatable symbols

   Definitions
      At line 102 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 55 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 103 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

SysTick_Handler 0000000C

Symbol: SysTick_Handler
   Definitions
      At line 110 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 59 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 111 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

TMR0_IRQHandler 0000000E

Symbol: TMR0_IRQHandler
   Definitions
      At line 137 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 67 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 121 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

TMR1_IRQHandler 0000000E

Symbol: TMR1_IRQHandler
   Definitions
      At line 138 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 68 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 122 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

TMR2_IRQHandler 0000000E

Symbol: TMR2_IRQHandler
   Definitions
      At line 139 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 69 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 123 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

TMRF_IRQHandler 0000000E




ARM Macro Assembler    Page 5 Alphabetic symbol ordering
Relocatable symbols

Symbol: TMRF_IRQHandler
   Definitions
      At line 144 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 74 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 128 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

USBD_IRQHandler 0000000E

Symbol: USBD_IRQHandler
   Definitions
      At line 136 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 66 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 120 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

WDT_IRQHandler 0000000E

Symbol: WDT_IRQHandler
   Definitions
      At line 132 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 62 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 116 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

__user_initial_stackheap 00000010

Symbol: __user_initial_stackheap
   Definitions
      At line 168 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      At line 167 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
Comment: __user_initial_stackheap used once
24 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Absolute symbols

Heap_Size 00000000

Symbol: Heap_Size
   Definitions
      At line 27 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 31 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 172 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

Stack_Size 00000100

Symbol: Stack_Size
   Definitions
      At line 16 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 19 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
      At line 171 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s

2 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
External symbols

__main 00000000

Symbol: __main
   Definitions
      At line 85 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
   Uses
      At line 86 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\startu
p_N572.s
Comment: __main used once
__use_two_region_memory 00000000

Symbol: __use_two_region_memory
   Definitions
      At line 166 in file ..\..\..\Library\Device\Nuvoton\N572\Source\ARM\start
up_N572.s
   Uses
      None
Comment: __use_two_region_memory unused
2 symbols
373 symbols in table
