Static Call Graph - [.\Objects\uipkernel_demo_stm32f103.axf]

# Static Call Graph for image .\Objects\uipkernel_demo_stm32f103.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Sat May 30 13:00:04 2020

### Maximum Stack Usage = 80 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ StartOS ⇒ uipAppInitialize ⇒ Kernel_System_Tick_Init ⇒ HAL_NVIC_SetPriority ⇒ NVIC_SetPriority

### Functions with no stack information

- __user_initial_stackheap
- uipDisableAllInterrupts
- uipIntMaskStateRestore
- uipPendSVHandler

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from chip_uip_interrupt.o(i.ADC1_2_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from chip_uip_interrupt.o(i.ADC3_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - AppIdleTask from demo.o(i.AppIdleTask) referenced 2 times from app_cfg.o(.data)
  - BusFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from chip_uip_interrupt.o(i.CAN1_RX1_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from chip_uip_interrupt.o(i.CAN1_SCE_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - Chip_UIP_InterruptNullHandler from chip_uip_interrupt.o(i.Chip_UIP_InterruptNullHandler) referenced from chip_uip_interrupt.o(i.Chip_UIP_InterruptInit)
  - DMA1_Channel1_IRQHandler from chip_uip_interrupt.o(i.DMA1_Channel1_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from chip_uip_interrupt.o(i.DMA1_Channel2_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from chip_uip_interrupt.o(i.DMA1_Channel3_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from chip_uip_interrupt.o(i.DMA1_Channel4_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from chip_uip_interrupt.o(i.DMA1_Channel5_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from chip_uip_interrupt.o(i.DMA1_Channel6_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from chip_uip_interrupt.o(i.DMA1_Channel7_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from chip_uip_interrupt.o(i.DMA2_Channel1_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from chip_uip_interrupt.o(i.DMA2_Channel2_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from chip_uip_interrupt.o(i.DMA2_Channel3_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from chip_uip_interrupt.o(i.DMA2_Channel4_5_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from chip_uip_interrupt.o(i.EXTI0_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from chip_uip_interrupt.o(i.EXTI15_10_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from chip_uip_interrupt.o(i.EXTI1_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from chip_uip_interrupt.o(i.EXTI2_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from chip_uip_interrupt.o(i.EXTI3_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from chip_uip_interrupt.o(i.EXTI4_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from chip_uip_interrupt.o(i.EXTI9_5_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from chip_uip_interrupt.o(i.FLASH_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from chip_uip_interrupt.o(i.FSMC_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from chip_uip_interrupt.o(i.I2C1_ER_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from chip_uip_interrupt.o(i.I2C1_EV_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from chip_uip_interrupt.o(i.I2C2_ER_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from chip_uip_interrupt.o(i.I2C2_EV_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from chip_uip_interrupt.o(i.PVD_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from chip_uip_interrupt.o(i.RCC_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from chip_uip_interrupt.o(i.RTCAlarm_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from chip_uip_interrupt.o(i.RTC_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from chip_uip_interrupt.o(i.SDIO_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from chip_uip_interrupt.o(i.SPI1_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from chip_uip_interrupt.o(i.SPI2_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from chip_uip_interrupt.o(i.SPI3_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x_cl.o(i.SystemInit) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from chip_uip_interrupt.o(i.TAMPER_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TASK_0 from demo.o(i.TASK_0) referenced 2 times from app_cfg.o(.data)
  - TASK_1 from demo.o(i.TASK_1) referenced 2 times from app_cfg.o(.data)
  - TASK_2 from demo.o(i.TASK_2) referenced 2 times from app_cfg.o(.data)
  - TASK_3 from demo.o(i.TASK_3) referenced 2 times from app_cfg.o(.data)
  - TASK_4 from demo.o(i.TASK_4) referenced 2 times from app_cfg.o(.data)
  - TIM1_BRK_IRQHandler from chip_uip_interrupt.o(i.TIM1_BRK_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from chip_uip_interrupt.o(i.TIM1_CC_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from chip_uip_interrupt.o(i.TIM1_TRG_COM_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from chip_uip_interrupt.o(i.TIM1_UP_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from chip_uip_interrupt.o(i.TIM2_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from chip_uip_interrupt.o(i.TIM3_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from chip_uip_interrupt.o(i.TIM4_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from chip_uip_interrupt.o(i.TIM5_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from chip_uip_interrupt.o(i.TIM6_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from chip_uip_interrupt.o(i.TIM7_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from chip_uip_interrupt.o(i.TIM8_BRK_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from chip_uip_interrupt.o(i.TIM8_CC_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from chip_uip_interrupt.o(i.TIM8_TRG_COM_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from chip_uip_interrupt.o(i.TIM8_UP_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from chip_uip_interrupt.o(i.UART4_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from chip_uip_interrupt.o(i.UART5_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from chip_uip_interrupt.o(i.USART1_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from chip_uip_interrupt.o(i.USART2_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from chip_uip_interrupt.o(i.USART3_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from chip_uip_interrupt.o(i.USBWakeUp_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from chip_uip_interrupt.o(i.USB_HP_CAN1_TX_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from chip_uip_interrupt.o(i.USB_LP_CAN1_RX0_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from chip_uip_interrupt.o(i.WWDG_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)
  - uipPendSVHandler from uip_kernel_isr_cm.o(CODE) referenced from startup_stm32f10x_hd.o(RESET)
  - uipSystemCounterHandler from uip_kernel_time.o(i.uipSystemCounterHandler) referenced from startup_stm32f10x_hd.o(RESET)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __decompress (Thumb, 90 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __decompress1 (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ StartOS ⇒ uipAppInitialize ⇒ Kernel_System_Tick_Init ⇒ HAL_NVIC_SetPriority ⇒ NVIC_SetPriority
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  uipDisableAllInterrupts (Thumb, 0 bytes, Stack size unknown bytes, uip_kernel_isr_cm.o(CODE))
  [Called By]

  - >> UIP_WaitEvent
  - >> UIP_TerminateTask
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource
  - >> UIP_ReceiveMessage
  - >> UIP_GetResource
  - >> UIP_ClearEvent
  - >> StartOS
  - >> uipInterruptServiceEngine
  - >> UIP_ActivateTask

  uipIntMaskStateRestore (Thumb, 0 bytes, Stack size unknown bytes, uip_kernel_isr_cm.o(CODE))
  [Called By]

  - >> UIP_WaitEvent
  - >> UIP_TerminateTask
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource
  - >> UIP_ReceiveMessage
  - >> UIP_GetResource
  - >> UIP_ClearEvent
  - >> StartOS
  - >> uipInterruptServiceEngine
  - >> UIP_ActivateTask

  uipPendSVHandler (Thumb, 0 bytes, Stack size unknown bytes, uip_kernel_isr_cm.o(CODE))
  [Stack]

  - Max Depth = 4 + Unknown Stack Size
  - Call Chain = uipPendSVHandler ⇒ uipPreContexSwitch
  [Calls]
  - >> uipPreContexSwitch
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.ADC1_2_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = ADC1_2_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.ADC3_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = ADC3_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  AppIdleTask (Thumb, 46 bytes, Stack size 0 bytes, demo.o(i.AppIdleTask))
  [Address Reference Count : 1]

  - app_cfg.o(.data)

  CAN1_RX1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.CAN1_RX1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = CAN1_RX1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.CAN1_SCE_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = CAN1_SCE_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  Chip_UIP_InterruptInit (Thumb, 36 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.Chip_UIP_InterruptInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_UIP_InterruptInit ⇒ Chip_UIP_InterruptRegisterHandler
  [Calls]
  - >> Chip_UIP_InterruptRegisterHandler
  [Called By]
  - >> Hardware_Init

  Chip_UIP_InterruptRegisterHandler (Thumb, 28 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.Chip_UIP_InterruptRegisterHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_UIP_InterruptRegisterHandler
  [Called By]
  - >> Chip_UIP_InterruptInit

  DMA1_Channel1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA1_Channel1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA1_Channel1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA1_Channel2_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA1_Channel2_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA1_Channel3_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA1_Channel3_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA1_Channel4_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA1_Channel4_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA1_Channel5_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA1_Channel5_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA1_Channel6_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA1_Channel6_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA1_Channel7_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA1_Channel7_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA2_Channel1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA2_Channel1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA2_Channel2_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA2_Channel2_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA2_Channel3_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA2_Channel3_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.DMA2_Channel4_5_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = DMA2_Channel4_5_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.EXTI0_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = EXTI0_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.EXTI15_10_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = EXTI15_10_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.EXTI1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = EXTI1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.EXTI2_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = EXTI2_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.EXTI3_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = EXTI3_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.EXTI4_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = EXTI4_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.EXTI9_5_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = EXTI9_5_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.FLASH_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = FLASH_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.FSMC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = FSMC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  HAL_NVIC_SetPriority (Thumb, 124 bytes, Stack size 40 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_NVIC_SetPriority ⇒ NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  - >> NVIC_GetPriorityGrouping
  [Called By]
  - >> Kernel_System_Tick_Init

  HAL_NVIC_SetPriorityGrouping (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> Hardware_Init

  HAL_RCC_GetHCLKFreq (Thumb, 42 bytes, Stack size 4 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> Kernel_System_Tick_Init

  HAL_RCC_GetSysClockFreq (Thumb, 146 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_GetHCLKFreq

  HAL_SYSTICK_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> Kernel_System_Tick_Init

  HAL_SYSTICK_Config (Thumb, 52 bytes, Stack size 16 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_SYSTICK_Config ⇒ NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> Kernel_System_Tick_Init

  Hardware_Init (Thumb, 54 bytes, Stack size 8 bytes, hardware_init.o(i.Hardware_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = Hardware_Init ⇒ Chip_UIP_InterruptInit ⇒ Chip_UIP_InterruptRegisterHandler
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> Chip_UIP_InterruptInit
  [Called By]
  - >> main

  I2C1_ER_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.I2C1_ER_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = I2C1_ER_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.I2C1_EV_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = I2C1_EV_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.I2C2_ER_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = I2C2_ER_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.I2C2_EV_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = I2C2_EV_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  InterruptHandler (Thumb, 78 bytes, Stack size 32 bytes, chip_uip_interrupt.o(i.InterruptHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = InterruptHandler
  [Called By]
  - >> uipInterruptHandlingCallback

  Kernel_System_Tick_Init (Thumb, 54 bytes, Stack size 8 bytes, hardware_init.o(i.Kernel_System_Tick_Init))
  [Stack]

  - Max Depth = 56
  - Call Chain = Kernel_System_Tick_Init ⇒ HAL_NVIC_SetPriority ⇒ NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> uipAppInitialize

  PVD_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.PVD_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = PVD_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.RCC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = RCC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.RTCAlarm_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = RTCAlarm_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.RTC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = RTC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.SDIO_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = SDIO_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.SPI1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = SPI1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.SPI2_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = SPI2_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.SPI3_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = SPI3_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  StartOS (Thumb, 38 bytes, Stack size 16 bytes, uip_kernel_common.o(i.StartOS))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = StartOS ⇒ uipAppInitialize ⇒ Kernel_System_Tick_Init ⇒ HAL_NVIC_SetPriority ⇒ NVIC_SetPriority
  [Calls]
  - >> uipAppInitialize
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  - >> uipKernelInitialize
  [Called By]
  - >> main

  SystemInit (Thumb, 386 bytes, Stack size 40 bytes, system_stm32f10x_cl.o(i.SystemInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = SystemInit ⇒ __aeabi_dmul
  [Calls]
  - >> __aeabi_dmul
  - >> __aeabi_i2d
  - >> __aeabi_d2uiz
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  TAMPER_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TAMPER_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TAMPER_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TASK_0 (Thumb, 22 bytes, Stack size 0 bytes, demo.o(i.TASK_0))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = TASK_0 ⇒ UIP_WaitEvent ⇒ uipGetNextTask
  [Calls]
  - >> UIP_WaitEvent
  - >> UIP_ClearEvent
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_1 (Thumb, 22 bytes, Stack size 0 bytes, demo.o(i.TASK_1))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = TASK_1 ⇒ UIP_WaitEvent ⇒ uipGetNextTask
  [Calls]
  - >> UIP_WaitEvent
  - >> UIP_ClearEvent
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_2 (Thumb, 32 bytes, Stack size 0 bytes, demo.o(i.TASK_2))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = TASK_2 ⇒ UIP_ReleaseResource ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_WaitEvent
  - >> UIP_ReleaseResource
  - >> UIP_GetResource
  - >> UIP_ClearEvent
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_3 (Thumb, 26 bytes, Stack size 0 bytes, demo.o(i.TASK_3))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = TASK_3 ⇒ UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource
  - >> UIP_GetResource
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TASK_4 (Thumb, 16 bytes, Stack size 16 bytes, demo.o(i.TASK_4))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = TASK_4 ⇒ UIP_ReceiveMessage
  [Calls]
  - >> UIP_TerminateTask
  - >> UIP_ReceiveMessage
  [Address Reference Count : 1]
  - app_cfg.o(.data)

  TIM1_BRK_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM1_BRK_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM1_BRK_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM1_CC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM1_CC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM1_TRG_COM_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM1_TRG_COM_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM1_UP_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM1_UP_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM2_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM2_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM3_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM3_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM4_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM4_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM5_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM5_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM6_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM6_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM7_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM7_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM8_BRK_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM8_BRK_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM8_CC_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM8_CC_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM8_TRG_COM_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM8_TRG_COM_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.TIM8_UP_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = TIM8_UP_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.UART4_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = UART4_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.UART5_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = UART5_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UIP_ActivateTask (Thumb, 220 bytes, Stack size 16 bytes, uip_kernel_task.o(i.UIP_ActivateTask))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = UIP_ActivateTask
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> uipAlarmHandler

  UIP_ClearEvent (Thumb, 68 bytes, Stack size 16 bytes, uip_kernel_event.o(i.UIP_ClearEvent))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = UIP_ClearEvent
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_2
  - >> TASK_1
  - >> TASK_0

  UIP_GetResource (Thumb, 162 bytes, Stack size 24 bytes, uip_kernel_resource.o(i.UIP_GetResource))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = UIP_GetResource
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_3
  - >> TASK_2

  UIP_ReceiveMessage (Thumb, 208 bytes, Stack size 32 bytes, uip_kernel_message.o(i.UIP_ReceiveMessage))
  [Stack]

  - Max Depth = 32 + Unknown Stack Size
  - Call Chain = UIP_ReceiveMessage
  [Calls]
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_4

  UIP_ReleaseResource (Thumb, 252 bytes, Stack size 32 bytes, uip_kernel_resource.o(i.UIP_ReleaseResource))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = UIP_ReleaseResource ⇒ uipGetNextPriority
  [Calls]
  - >> uipGetNextPriority
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_3
  - >> TASK_2

  UIP_SetEvent (Thumb, 268 bytes, Stack size 32 bytes, uip_kernel_event.o(i.UIP_SetEvent))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> uipGetNextPriority
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_3
  - >> uipAlarmHandler

  UIP_TerminateTask (Thumb, 228 bytes, Stack size 16 bytes, uip_kernel_task.o(i.UIP_TerminateTask))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = UIP_TerminateTask ⇒ uipGetNextTask
  [Calls]
  - >> uipGetNextTask
  - >> uipClearPrioGrpAndArrayBit
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  - >> uipTaskStackInit
  [Called By]
  - >> TASK_4

  UIP_WaitEvent (Thumb, 118 bytes, Stack size 16 bytes, uip_kernel_event.o(i.UIP_WaitEvent))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = UIP_WaitEvent ⇒ uipGetNextTask
  [Calls]
  - >> uipGetNextTask
  - >> uipClearPrioGrpAndArrayBit
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> TASK_2
  - >> TASK_1
  - >> TASK_0

  USART1_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = USART1_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.USART2_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = USART2_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.USART3_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = USART3_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.USBWakeUp_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = USBWakeUp_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.USB_HP_CAN1_TX_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = USB_HP_CAN1_TX_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.USB_LP_CAN1_RX0_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = USB_LP_CAN1_RX0_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.WWDG_IRQHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = WWDG_IRQHandler ⇒ uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptServiceEngine
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  main (Thumb, 22 bytes, Stack size 0 bytes, demo.o(i.main))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = main ⇒ StartOS ⇒ uipAppInitialize ⇒ Kernel_System_Tick_Init ⇒ HAL_NVIC_SetPriority ⇒ NVIC_SetPriority
  [Calls]
  - >> StartOS
  - >> Hardware_Init
  [Called By]
  - >> __rt_entry_main

  uipAlarmHandler (Thumb, 116 bytes, Stack size 16 bytes, uip_kernel_time.o(i.uipAlarmHandler))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = uipAlarmHandler ⇒ UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> UIP_SetEvent
  - >> UIP_ActivateTask
  [Called By]
  - >> uipSystemCounterHandler

  uipAlarmInitialize (Thumb, 34 bytes, Stack size 0 bytes, uip_kernel_common.o(i.uipAlarmInitialize))
  [Called By]

  - >> uipAppInitialize

  uipAppInitialize (Thumb, 60 bytes, Stack size 8 bytes, demo.o(i.uipAppInitialize))
  [Stack]

  - Max Depth = 64
  - Call Chain = uipAppInitialize ⇒ Kernel_System_Tick_Init ⇒ HAL_NVIC_SetPriority ⇒ NVIC_SetPriority
  [Calls]
  - >> uipTaskInitialize
  - >> uipResInitialize
  - >> uipMsgInitialize
  - >> uipAlarmInitialize
  - >> Kernel_System_Tick_Init
  [Called By]
  - >> StartOS

  uipClearPrioGrpAndArrayBit (Thumb, 96 bytes, Stack size 8 bytes, uip_kernel_scheduler.o(i.uipClearPrioGrpAndArrayBit))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipClearPrioGrpAndArrayBit
  [Called By]
  - >> UIP_WaitEvent
  - >> UIP_TerminateTask

  uipGetNextPriority (Thumb, 74 bytes, Stack size 8 bytes, uip_kernel_scheduler.o(i.uipGetNextPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipGetNextPriority
  [Called By]
  - >> UIP_SetEvent
  - >> UIP_ReleaseResource

  uipGetNextTask (Thumb, 120 bytes, Stack size 8 bytes, uip_kernel_scheduler.o(i.uipGetNextTask))
  [Stack]

  - Max Depth = 8
  - Call Chain = uipGetNextTask
  [Called By]
  - >> UIP_WaitEvent
  - >> UIP_TerminateTask
  - >> uipInterruptServiceEngine

  uipInterruptHandlingCallback (Thumb, 20 bytes, Stack size 8 bytes, chip_uip_interrupt.o(i.uipInterruptHandlingCallback))
  [Stack]

  - Max Depth = 40
  - Call Chain = uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> InterruptHandler
  [Called By]
  - >> uipInterruptServiceEngine

  uipInterruptServiceEngine (Thumb, 252 bytes, Stack size 8 bytes, uip_kernel_isr_engine.o(i.uipInterruptServiceEngine))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = uipInterruptServiceEngine ⇒ uipInterruptHandlingCallback ⇒ InterruptHandler
  [Calls]
  - >> uipInterruptHandlingCallback
  - >> uipGetNextTask
  - >> uipIntMaskStateRestore
  - >> uipDisableAllInterrupts
  [Called By]
  - >> WWDG_IRQHandler
  - >> USB_LP_CAN1_RX0_IRQHandler
  - >> USB_HP_CAN1_TX_IRQHandler
  - >> USBWakeUp_IRQHandler
  - >> USART3_IRQHandler
  - >> USART2_IRQHandler
  - >> USART1_IRQHandler
  - >> UART5_IRQHandler
  - >> UART4_IRQHandler
  - >> TIM8_UP_IRQHandler
  - >> TIM8_TRG_COM_IRQHandler
  - >> TIM8_CC_IRQHandler
  - >> TIM8_BRK_IRQHandler
  - >> TIM7_IRQHandler
  - >> TIM6_IRQHandler
  - >> TIM5_IRQHandler
  - >> TIM4_IRQHandler
  - >> TIM3_IRQHandler
  - >> TIM2_IRQHandler
  - >> TIM1_UP_IRQHandler
  - >> TIM1_TRG_COM_IRQHandler
  - >> TIM1_CC_IRQHandler
  - >> TIM1_BRK_IRQHandler
  - >> TAMPER_IRQHandler
  - >> SPI3_IRQHandler
  - >> SPI2_IRQHandler
  - >> SPI1_IRQHandler
  - >> SDIO_IRQHandler
  - >> RTC_IRQHandler
  - >> RTCAlarm_IRQHandler
  - >> RCC_IRQHandler
  - >> PVD_IRQHandler
  - >> I2C2_EV_IRQHandler
  - >> I2C2_ER_IRQHandler
  - >> I2C1_EV_IRQHandler
  - >> I2C1_ER_IRQHandler
  - >> FSMC_IRQHandler
  - >> FLASH_IRQHandler
  - >> EXTI9_5_IRQHandler
  - >> EXTI4_IRQHandler
  - >> EXTI3_IRQHandler
  - >> EXTI2_IRQHandler
  - >> EXTI1_IRQHandler
  - >> EXTI15_10_IRQHandler
  - >> EXTI0_IRQHandler
  - >> DMA2_Channel4_5_IRQHandler
  - >> DMA2_Channel3_IRQHandler
  - >> DMA2_Channel2_IRQHandler
  - >> DMA2_Channel1_IRQHandler
  - >> DMA1_Channel7_IRQHandler
  - >> DMA1_Channel6_IRQHandler
  - >> DMA1_Channel5_IRQHandler
  - >> DMA1_Channel4_IRQHandler
  - >> DMA1_Channel3_IRQHandler
  - >> DMA1_Channel2_IRQHandler
  - >> DMA1_Channel1_IRQHandler
  - >> CAN1_SCE_IRQHandler
  - >> CAN1_RX1_IRQHandler
  - >> ADC3_IRQHandler
  - >> ADC1_2_IRQHandler

  uipKernelInitialize (Thumb, 188 bytes, Stack size 0 bytes, uip_kernel_common.o(i.uipKernelInitialize))
  [Called By]

  - >> StartOS

  uipMsgInitialize (Thumb, 62 bytes, Stack size 12 bytes, uip_kernel_common.o(i.uipMsgInitialize))
  [Stack]

  - Max Depth = 12
  - Call Chain = uipMsgInitialize
  [Called By]
  - >> uipAppInitialize

  uipPreContexSwitch (Thumb, 68 bytes, Stack size 4 bytes, uip_kernel_scheduler.o(i.uipPreContexSwitch))
  [Stack]

  - Max Depth = 4
  - Call Chain = uipPreContexSwitch
  [Calls]
  - >> uipResetPrioGrpAndArrayBit
  [Called By]
  - >> uipPendSVHandler

  uipResInitialize (Thumb, 76 bytes, Stack size 12 bytes, uip_kernel_common.o(i.uipResInitialize))
  [Stack]

  - Max Depth = 12
  - Call Chain = uipResInitialize
  [Called By]
  - >> uipAppInitialize

  uipResetPrioGrpAndArrayBit (Thumb, 62 bytes, Stack size 0 bytes, uip_kernel_scheduler.o(i.uipResetPrioGrpAndArrayBit))
  [Called By]

  - >> uipPreContexSwitch

  uipSystemCounterHandler (Thumb, 116 bytes, Stack size 16 bytes, uip_kernel_time.o(i.uipSystemCounterHandler))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = uipSystemCounterHandler ⇒ uipAlarmHandler ⇒ UIP_SetEvent ⇒ uipGetNextPriority
  [Calls]
  - >> uipAlarmHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  uipTaskInitialize (Thumb, 236 bytes, Stack size 20 bytes, uip_kernel_common.o(i.uipTaskInitialize))
  [Stack]

  - Max Depth = 20
  - Call Chain = uipTaskInitialize
  [Calls]
  - >> uipTaskStackInit
  [Called By]
  - >> uipAppInitialize

  uipTaskStackInit (Thumb, 76 bytes, Stack size 0 bytes, uip_kernel_common.o(i.uipTaskStackInit))
  [Called By]

  - >> uipTaskInitialize
  - >> UIP_TerminateTask

  __aeabi_d2uiz (Thumb, 0 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2uiz
  [Called By]
  - >> SystemInit

  _dfixu (Thumb, 90 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu), UNUSED)
  [Calls]

  - >> __fpl_dnaninf

  __aeabi_i2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt))
  [Called By]

  - >> SystemInit

  _dflt (Thumb, 46 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt), UNUSED)

  __aeabi_dmul (Thumb, 0 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_dmul
  [Called By]
  - >> SystemInit

  _dmul (Thumb, 332 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf), UNUSED)
  [Called By]

  - >> _dmul
  - >> _dfixu

  __fpl_dretinf (Thumb, 12 bytes, Stack size 0 bytes, dretinf.o(x$fpl$dretinf), UNUSED)
  [Called By]

  - >> _dmul

  ### Local Symbols

  Chip_UIP_InterruptNullHandler (Thumb, 4 bytes, Stack size 0 bytes, chip_uip_interrupt.o(i.Chip_UIP_InterruptNullHandler))
  [Address Reference Count : 1]

  - chip_uip_interrupt.o(i.Chip_UIP_InterruptInit)

  NVIC_GetPriorityGrouping (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.NVIC_GetPriorityGrouping))
  [Called By]

  - >> HAL_NVIC_SetPriority

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_SetPriority
  [Called By]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  ### Undefined Global Symbols